FERMILAB-Conf-97/140 CBPF-NT-03/97

WWW Oriented Remote Job Submission, Monitoring and Management over Internet

G.A. Alves^a, M. Jofőly^{a,b}, M. Miranda^a, A. Santoro^{a,b} and M.H.G. Souza^a

a LAFEX/CBPF R. Dr. Xavier Sigaud, 150 Rio de Janeiro, RJ, Brazil

b Fermi National Accelerator Laboratory P.O. Box 500, Batavia, Illinois 60510

May 1997

Published Proceedings of CHEP 97, Berlin, Germany, April 7-11, 1997

Operated by Universities Research Association Inc. under Contract No. DE-AC02-76CH03000 with the United States Department of Energy

Disclaimer

This report was prepared as an account of work sponsored by an agency of the United States Government. Neither the United States Government nor any agency thereof, nor any of their employees, makes any warranty, expressed or implied, or assumes any legal liability or responsibility for the accuracy, completeness, or usefulness of any information, apparatus, product, or process disclosed, or represents that its use would not infringe privately owned rights. Reference herein to any specific commercial product, process, or service by trade name, trademark, manufacturer, or otherwise, does not necessarily constitute or imply its endorsement, recommendation, or favoring by the United States Government or any agency thereof. The views and opinions of authors expressed herein do not necessarily state or reflect those of the United States Government or any agency thereof.

Distribution

Approved for public release; further dissemination unlimited.

WWW Oriented Remote Job Submission, Monitoring and Management over Internet

G. A. Alves^{a;1}, M. Joffily^{a;b}, M. Miranda^a, A. Santoro^{a;b}, M. H. G. Souza^a

a LAFEX/CBPF R. Dr. Xavier Sigaud, 150 Rio de Janeiro, RJ, Brazil b Fermilab P.O.Box 500, Batavia, Il 60510, USA

We present a system which allows job submission over Internet with reliable data transfer using WWW graphical interface for job submission and monitoring and job management. Key words: Network; Parallel Processing; WWW; Computing Farms

1 Introduction

The growing need for computational resources in big collaborations like Dffl Zeus and LHC leads to the use of resources located in di¸erent sites. We have developed a system that allows one to submit and monitor a job over Internet using a WWW Interface. The system assumes there is a centralized server which receives job requests and sends them over Internet to a production site. The centralized server also functions like a temporary archiver for the input and output data.

The system is conceived to be used in any kind of job with the following characteristics:

{ CPU intensive { event oriented, with uncorrelated events

1 gilvan@lafex.cbpf.br

Preprint submitted to Elsevier Preprint 5 June 1997

{ 1 input and 1 output event ˛le (possible very large), besides calibration and control ˛les

It is also assumed that the production site has been properly con˛gured with calibration, control and other data ˛les as well as any environment parameters. Also, the executable program must be available in the production site.

The system can be used for any program with the characteristics mentioned earlier. It can easily be customized, if required, to accommodate speci˛c requirements of a particular system. Among the customizations that we can envision are elements for priorities, permissions, and parameters for the job. However, in most cases, almost no customization is required.

The system is composed of two main parts that will be explained in the following sections: the submission and monitoring system and the core system which implements the reliable data transfer and job control.

2 The Submission, Monitoring and Management System

The submission and monitoring system is based on a WWW interface, as is the Management interface.

The submission system is layered in a three-tier architecture: a HTML page that holds the GUI, a CGI-BIN program that handles the requests generated by the user and makes entries in a requisition ˛le and ˛nally a daemon that controls the job submission.

The user submits a job by connecting to the WWW server in the Central Server. Information such as input data ˛le, job parameters, user identi˛cation and priority are sent to the server, where the CGI-BIN program generates an entry in a request ˛le. The submission daemon constantly examines the requests and starts the job when there is a production system available. Policies such as priority and user privileges can be customized. For such customization, a routine has to be written. A template with a FIFO policy is distributed with the system.

Once a job is selected for execution, the submission system starts the core system which in turn starts the job on the designated site. At the end of the job, the user is noti˛ed by e-mail.

Every job submitted receives a JobId which is used for monitoring the job. To monitor a job, the user connects to the status page of the WWW server. The monitoring system will tell if the job is waiting, running or ˛nished. If the job is running, further information can be provided such as number of events already processed, status of the farm, and others. Also, it is possible to monitor the state of each CPU de˛ned for a farm.

The management system allows one to check a speci˛c node, add and remove nodes from a farm. The core system allows recon˛guration of the production site without having to stop any running job. By using the management interface, the manager of the site can add or remove nodes on the ‚y. When a node is removed, it ˛nishes the processing of the event it is eventually working on, and then it is removed from the farm.

3 The Core System

The Core scheme, written in C++, implements IO Classes to deal with Event gathering, transmission, and submission. The primary ingredients are the IO Objects which are de˛ned as entities that carry ONE Event. They have three main \properties": a Bu¸er, where Event data are stored, a Byte Count that gives the actual size of the Event and an IO Channel which identi˛es the IO device where data will be read/write, which can be ˛le descriptors, pipes, Sockets, etc. We can think them as a Class, which in C –++ Language will read:

class io˙operations – // This class defines objects with signatures: protected:

char *buf;

int io˙chan; (or struct sockadd sock, for Sockets) int count;

// and methods acting upon : public:

io˙operations (char *path, char *type); //Constructor ~io˙operations (void); //Destructor

void set˙buffer(char *new˙buf, int new˙count); char *get˙buffer(void) –return buf;˝ int get˙count(void) – return count;˝

void get˙dat(void); void send˙dat(void); ˝; These objects will be doing some IO, either reading ONE event and storing it on bu¸er, or writing ONE event from the bu¸er, from/to an IO device, which can be disk ˛le, a Named Pipe or BSD Sockets.

As can be seen from the above code template, this information is protected (encapsulated) from outside the Class scope. Methods are de˛ned for a standard access to it, from outside. They are:

{ Every time a Class member is de˛ned, a Constructor method is invoked.

It does all task of initialization, among them, an io channel is opened. The argument path will indicate a location, for instance, a ˛le name together of the directory or can be a pipe name or a BSD Socket structure. The second argument type will indicate when we will be doing reading or writing tasks. ( Actually, in our implementation, we use di¸erent Sub-classes for each task, all inheriting the properties of the basic IO Class io operations ).

In each case, the implementation is able, from these arguments, to make the correct identi˛cation of the device type and do everything needed to open it.

{ Methods are de˛ned to access encapsulated data in a standard protected way, for instance, the Event bu¸er: char *get buffer(void) .

{ Also, Methods are de˛ned to make the appropriate IO operation: get dat and send dat . When reading, the bu¸er will be dynamically allocated in virtual memory. Of course, these methods should be able to know about the event size. Also, they must know how to deal with di¸erent possibilities, other than experiment formats, following the IO device types.

An example template that will read data in some prede˛ned format from tape and will write them to a Named Pipe, can be read as:

#include ... // whatever includes you need #include ”io˙header.h” // IO Class definitions include file main() – class io˙operations tape1(”/dev/rmt0”, ”READ”); class io˙operations tape10(”/local/userb/disk.dat”, ”WRITE”);

tape1.options(”E740”); tape10.options(”PIPE”);

for (int k = 0 ; k ¡ event ; k++) –

tape1.get˙dat();

cout ¡¡ ”Read phase byte count: ” ¡¡ tape1.get˙count() ¡¡ ”“n”;

tape10.set˙buffer( tape1.get˙buffer(), tape1.get˙count()); tape10.send˙dat(); ˝ ˝

With the above de˛ned IO Classes, we construct IO Modules, which will be the building blocks of the system. They are basically IO loops, following pretty much the above skeleton. There are two kinds of such modules:

{ Client Modules read data available on Named Pipes or on disk ˛les. To read each Event , an IO object will be created, which will hand over it to another IO object to carry this event and write it to a Socket.

{ Server Modules are always alive, watching for incoming data on Sockets.

When data is available on a socket, IO objects are created, again on an event basis. When downstream Named Pipes are ready to accept events (which means that a Client Module is ready to accept data on the other side of the pipe), then another IO objects are activated to transmit them. This mechanism is the core of how the system does work: each event in each module is dealt by 2 di¸erent objects. When input data is present, objects will store them in virtual memory. When downstream IO is possible, then and only then, objects will be created to do data transmission. All allocations will be free and all objects destroyed.

From the core point of view, there are 3 elements: Central site, Server site and nodes.

{ Nodes are CPUs that actually run the programs ( huge fortran programs consuming several minutes of CPU time), expect input data (some hundreds of MB) and produce output data of same order of magnitude. Data is made available on Unix Sockets.

{ At the Server site ( a Unix machine ) a ˛le, LOCAL RESOURCES, de- ˛nes completely the farm. The same server programs above are used to read input data (from the Central Site) on sockets, write it on named pipes, which are read by the client programs and shipped out to nodes ( de- ˛ned in LOCAL RESOURCES ) via Unix sockets. On the other hand, the server programs listen to sockets for returning data from nodes, write it on named pipes, which are read by client programs, in the same way as before. Data are then shipped back to Central Site. In short, there are 4 Client/Server programs running in this site ( the same two binaries, with di¸erent parameters ). They are all blocked on pipes and sockets, in absence of incoming/outgoing data. Once nodes need data or outgoing data is present on a socket, the transmission is made, on an event by event basis.

{ Jobs are submitted from a Central Site, which may or may not be an Archive Site.

This model is very ‚exible for dealing with a variable ‚ux of data. We should remember that each event is produced at a rate of (some) minutes/event and so, all overhead in making IO on intermediate ˛fos and sockets is negligible. So, in a normal scenario, we will have only one event transmitted over this system. Suppose now that several connections are made, each from a location that runs

Monte-Carlo jobs. Several of these requests can arrive simultaneously. In this case, this ‚exibility shows its best qualities: all data will be accepted by the Server, freeing the upstream systems to resume its jobs with new fresh input. Data will then be transmitted from the Server to the Client through the ˛fo, on a steady event by event basis.

The system can catch and recover from Internet time-outs, broken pipes and so forth, without loosing events. The system also can sense and recover from node program crashes automatically. In this case, only the faulty event is lost.

4 Virtual Farms

It is worth pointing out that the Central Manager and the Production site can be any UNIX machine connected through Internet. This means that one can build a local System using the available workstations. If the program’s priorities are set low, one can build a production system using the otherwise unused cycles of the workstations on this institution. The nodes of the system can also be spread over the world, making a "Virtual Farm". Because it is assumed that the programs are CPU intensive, little load should be put on the network.

5 Conclusion

A pilot system is running now at Fermilab, as part of the overall Monte Carlo simulation e¸ort of the Dffl experiment.

Prior experience in working with farms and farm’s software, such as CPS [1] and Funnel [2], in‚uenced this project. In particular, many good ideas were borrowed from Funnel.

This project added to the successful CPS and Funnel projects the following characteristics:

{ Object Oriented approach;

{ Fault Tolerance in regard to network problems;

{ GUI for job submission and monitoring and system management using WWW.

A last remark is that this system takes advantage of the lack of correlation between event processing, and allows the use of unmodi˛ed sequential application programs.

6 Acknowledgements

We would like to thank FINEP/Brazil and IBM/Brazil for ˛nancial support to build up the computer farm in which this software was developed. Two of us, A.S. and M.J., would like to thank the Computing Division/Fermilab for the hospitality.

References

[1] F. Rinaldo and S. Wolbers, Loosely Coupled Parallel Processing at Fermilab , Computer in Physics, vol. 7, no.2 (1993) 184

[2] B. Burow, Funnel: Towards Comfortable Event Processing, Proceedings of Computing in High Energy Physics, CHEP95, Rio de Janeiro, 18-22 Sept. 1995